**MONITOR 2.0 SPECIFICATIONS**

1. Memory Organization

FFFF-----------------------

BIOS (same as CP/M)

E600-----------------------

MONITOR

D000-----------------------

TPA

0100-----------------------

PZERO (same as CP/M)

0000-----------------------

1. Commands

* MEMO – memory operations
* RUN – execute a program
* XMODEM – receive a file
* HEX2COM – convert hex file to executable
* LCD – write on LCD
* DISK – disk operations
  1. MEMO

M>? Show help.

M>^C Exit command (return to Monitor).

M>Raaaa Read one page, starting at aaaa.

<ENTER>=Next page, <ESC>=quit.

M>Waaaa Write starting at aaaa. End

sequence with <ENTER>.

M>Faaaa-bbbb,cc Fill area aaaa till bbbb with cc.

M>Caaaa-bbbb,cccc Copy area aaaa till bbbb to cccc.

M>Vaaaa-bbbb Verify integrity of area from aaaa

to bbbb.

M>Saaaa-bbbb,c1c2…cN Search for the sequence in the

Saaaa-bbbb,"string" range aaaa to bbbb.

* 1. RUN

>RUNaaaa Execute program at aaaa. (aaaa must be in TPA)

* 1. XMODEM

>XMODEM aaaa Receive a file, using xmodem protocol, and

save at aaaa.

* 1. HEX2COM

>HEX2COM aaaa Convert HEX file (Intel format) at aaaa

to executable.

* 1. LCD

L>Paaaa,d Print on LCD text starting at aaaa, finishing

with 00 character. Use d seconds delay between

each line. <ESC> to quit.

L>W Enter WYSIWYG window. Use arrows to navigate,

^H to clear LCD, and <ESC> to quit.

* 1. DISK

Disk operations are addressed using DTS format (Disk, Track, Sector). In order to keep compatibility with CP/M 128MB Flash, these are the physical limits:

* Disk in range [A; P] (16 disks)
* Track in range [000; 1FF] (512 tracks/disk)
* Sector in range [00; 1F] (32 sectors/track)

(512 bytes/sector)

D>? Show help.

D>^C Exit command (return to Monitor).

D>Rd,ttt,ss Read one sector, starting at the

specified location (d,ttt,ss).

<ENTER>=next sector, <ESC>=quit.

D>Cd,ttt,ss-aaaa Copy one sector from d,ttt,ss to

memory aaaa.

D>Caaaa-d,ttt,ss Copy one sector from memory aaaa to

disk location d,ttt,ss.

D>Vd,ttt,ss Verify sector d,ttt,ss.

Vd,ttt Verify all sectors in track d,ttt.

Vd Verify all sectors in disk d.

Vfull Verify full media.

XXXXX – phase 1

XXXXX – phase 2

XXXXX – phase 3

XXXXX – not sure if needed